|  |  |
| --- | --- |
| Front: **Routers**  **OBJ 2.2** | Front: **Switches**  **OBJ 2.2** |
| Front: **Wireless Access Point (WAP)**  **OBJ 2.2** | Front: **Patch Panel**  **OBJ 2.2** |
| Front: **Firewall**  **OBJ 2.2** | Front: **Power Over Ethernet (PoE)**  **OBJ 2.2** |

|  |  |
| --- | --- |
| Back: **refer to the ObsidianMD / Anki notes** | Back: **- used to connect different networks together** |
| Back:  **- device that allows cable networks jacks**  **from a wall into a central area** | Back: **- Device that allows wireless devices to**  **connect to a wired network** |
| Back:  **refer to the ObsidianMD / Anki notes** | Back:  **- Scans and blocks traffic that enters or leaves**  **a network**  **- unified threat management (UTM) contains**  **firewall features** |